**[FT-P200SMZ](javascript:getCans(6631,1))**

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
| **Camera** |  |  |
| Image Sensor: | | | 2MP  Progressive Scan CMOS |
| Signal System: | | | PAL/NTSC |
| Lens: | | | 3.6mm lens |
| Lens Mount: | | | M10 |
| Day& Night: | | | IR cut filter with auto switch |
| **Compression  Standard** |  |  |
| Video Compression: | | | H.264/MJPEG |
| Video bit rate | | | 32Kbps~8Mbps |
| Triple Streams: | | | No |
| **Image** |  |  |
| Max. Image Resolution: | | | 1920x1080 |
| Frame Rate: | | | 1080P@6fps |
| **Network** |  |  |
| General Function: | | | The outer TF card slot, the biggest can support 128g、Support motion detection,、alarm push and linkage、JPEG snapshot,、support iCSee Application Center. |
| System Compatibility: | | | Support WiFi/wired |
| **General** |  |  |
| Operating Conditions: | | | -10 °C ~ 60 °C (14 °F ~ 140 °F) Humidity 90% or less (non-condensing) |
| Power Supply: | | | 5V micro USB |
| Weather Proof: | | | IP65 |
| IR Range: | | | Up to 15m |
| Dimensions: | | | 109×83mm |
| Weight: | | | 850g |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |